;
;
; Installs WinUsb
;

[Version]
Signature = "$Windows NT$"
Class     = KmWinUSB
ClassGUID = {F3ACB5C9-5685-4f07-96B5-89C5B22CB436}
Provider  = %ManufacturerName%
CatalogFile = KmWinUSB1.cat
DriverVer=09/04/2012,13.54.20.543

; ========== Manufacturer/Models sections ===========

[Manufacturer]
%ManufacturerName% = KDCWINUSB,NTx86.6.0,NTamd64.6.0

[KDCWINUSB.NTx86.6.0]
Kyocera CS 2552ci = USB_Install, USB\VID_0482&PID_06d5&MI_01
Kyocera CS 2552ci = USB_Install, USB\VID_0482&PID_06d5&MI_02
Kyocera CS 3252ci = USB_Install, USB\VID_0482&PID_06d4&MI_01
Kyocera CS 3252ci = USB_Install, USB\VID_0482&PID_06d4&MI_02
Kyocera CS 3552ci = USB_Install, USB\VID_0482&PID_0c35&MI_01
Kyocera CS 3552ci = USB_Install, USB\VID_0482&PID_0c35&MI_02
Kyocera CS 4002i = USB_Install, USB\VID_0482&PID_06d8&MI_01
Kyocera CS 4002i = USB_Install, USB\VID_0482&PID_06d8&MI_02
Kyocera CS 4052ci = USB_Install, USB\VID_0482&PID_06d3&MI_01
Kyocera CS 4052ci = USB_Install, USB\VID_0482&PID_06d3&MI_02
Kyocera CS 5002i = USB_Install, USB\VID_0482&PID_06d7&MI_01
Kyocera CS 5002i = USB_Install, USB\VID_0482&PID_06d7&MI_02
Kyocera CS 5052ci = USB_Install, USB\VID_0482&PID_06d2&MI_01
Kyocera CS 5052ci = USB_Install, USB\VID_0482&PID_06d2&MI_02
Kyocera CS 6002i = USB_Install, USB\VID_0482&PID_06d6&MI_01
Kyocera CS 6002i = USB_Install, USB\VID_0482&PID_06d6&MI_02
Kyocera CS 6052ci = USB_Install, USB\VID_0482&PID_06d1&MI_01
Kyocera CS 6052ci = USB_Install, USB\VID_0482&PID_06d1&MI_02
Kyocera CS 7002i = USB_Install, USB\VID_0482&PID_06dc&MI_01
Kyocera CS 7002i = USB_Install, USB\VID_0482&PID_06dc&MI_02
Kyocera CS 7052ci = USB_Install, USB\VID_0482&PID_06da&MI_01
Kyocera CS 7052ci = USB_Install, USB\VID_0482&PID_06da&MI_02
Kyocera CS 8002i = USB_Install, USB\VID_0482&PID_06db&MI_01
Kyocera CS 8002i = USB_Install, USB\VID_0482&PID_06db&MI_02
Kyocera CS 8052ci = USB_Install, USB\VID_0482&PID_06d9&MI_01
Kyocera CS 8052ci = USB_Install, USB\VID_0482&PID_06d9&MI_02
Kyocera ECOSYS M2040dn = USB_Install, USB\VID_0482&PID_069d&MI_02
Kyocera ECOSYS M2135dn = USB_Install, USB\VID_0482&PID_069a&MI_02
Kyocera ECOSYS M2540dn = USB_Install, USB\VID_0482&PID_06fd&MI_02
Kyocera ECOSYS M2540dw = USB_Install, USB\VID_0482&PID_069e&MI_02
Kyocera ECOSYS M2635dn = USB_Install, USB\VID_0482&PID_069b&MI_02
Kyocera ECOSYS M2635dw = USB_Install, USB\VID_0482&PID_069c&MI_02
Kyocera ECOSYS M2640idw = USB_Install, USB\VID_0482&PID_069f&MI_02
Kyocera ECOSYS M2735dw = USB_Install, USB\VID_0482&PID_06fe&MI_02
Kyocera ECOSYS M5520cdn = USB_Install, USB\VID_0482&PID_0c18&MI_02
Kyocera ECOSYS M5520cdw = USB_Install, USB\VID_0482&PID_0c17&MI_02
Kyocera ECOSYS M5521cdn = USB_Install, USB\VID_0482&PID_06b1&MI_02
Kyocera ECOSYS M5521cdw = USB_Install, USB\VID_0482&PID_06b2&MI_02
Kyocera ECOSYS M5525cdn = USB_Install, USB\VID_0482&PID_0c16&MI_02
Kyocera ECOSYS M5526cdn = USB_Install, USB\VID_0482&PID_06b3&MI_02
Kyocera ECOSYS M5526cdw = USB_Install, USB\VID_0482&PID_06b4&MI_02
Kyocera ECOSYS P2040dn = USB_Install, USB\VID_0482&PID_0698&MI_01
Kyocera ECOSYS P2040dw = USB_Install, USB\VID_0482&PID_0699&MI_01
Kyocera ECOSYS P2235dn = USB_Install, USB\VID_0482&PID_0696&MI_01
Kyocera ECOSYS P2235dw = USB_Install, USB\VID_0482&PID_0697&MI_01
Kyocera ECOSYS P3045dn = USB_Install, USB\VID_0482&PID_0c2d&MI_01
Kyocera ECOSYS P3050dn = USB_Install, USB\VID_0482&PID_0c2c&MI_01
Kyocera ECOSYS P3055dn = USB_Install, USB\VID_0482&PID_0c2b&MI_01
Kyocera ECOSYS P3060dn = USB_Install, USB\VID_0482&PID_0c2a&MI_01
Kyocera ECOSYS P5020cdn = USB_Install, USB\VID_0482&PID_0c15&MI_01
Kyocera ECOSYS P5020cdw = USB_Install, USB\VID_0482&PID_0c14&MI_01
Kyocera ECOSYS P5021cdn = USB_Install, USB\VID_0482&PID_06ad&MI_01
Kyocera ECOSYS P5021cdw = USB_Install, USB\VID_0482&PID_06ae&MI_01
Kyocera ECOSYS P5025cdn = USB_Install, USB\VID_0482&PID_0c13&MI_01
Kyocera ECOSYS P5026cdn = USB_Install, USB\VID_0482&PID_06af&MI_01
Kyocera ECOSYS P5026cdw = USB_Install, USB\VID_0482&PID_06b0&MI_01
Kyocera TASKalfa 2552ci = USB_Install, USB\VID_0482&PID_06c1&MI_01
Kyocera TASKalfa 2552ci = USB_Install, USB\VID_0482&PID_06c1&MI_02
Kyocera TASKalfa 3252ci = USB_Install, USB\VID_0482&PID_06c0&MI_01
Kyocera TASKalfa 3252ci = USB_Install, USB\VID_0482&PID_06c0&MI_02
Kyocera TASKalfa 3552ci = USB_Install, USB\VID_0482&PID_0c34&MI_01
Kyocera TASKalfa 3552ci = USB_Install, USB\VID_0482&PID_0c34&MI_02
Kyocera TASKalfa 4002i = USB_Install, USB\VID_0482&PID_06d0&MI_01
Kyocera TASKalfa 4002i = USB_Install, USB\VID_0482&PID_06d0&MI_02
Kyocera TASKalfa 4052ci = USB_Install, USB\VID_0482&PID_06bf&MI_01
Kyocera TASKalfa 4052ci = USB_Install, USB\VID_0482&PID_06bf&MI_02
Kyocera TASKalfa 5002i = USB_Install, USB\VID_0482&PID_06c3&MI_01
Kyocera TASKalfa 5002i = USB_Install, USB\VID_0482&PID_06c3&MI_02
Kyocera TASKalfa 5052ci = USB_Install, USB\VID_0482&PID_06be&MI_01
Kyocera TASKalfa 5052ci = USB_Install, USB\VID_0482&PID_06be&MI_02
Kyocera TASKalfa 6002i = USB_Install, USB\VID_0482&PID_06c2&MI_01
Kyocera TASKalfa 6002i = USB_Install, USB\VID_0482&PID_06c2&MI_02
Kyocera TASKalfa 6052ci = USB_Install, USB\VID_0482&PID_06bd&MI_01
Kyocera TASKalfa 6052ci = USB_Install, USB\VID_0482&PID_06bd&MI_02
Kyocera TASKalfa 7002i = USB_Install, USB\VID_0482&PID_06c7&MI_01
Kyocera TASKalfa 7002i = USB_Install, USB\VID_0482&PID_06c7&MI_02
Kyocera TASKalfa 7052ci = USB_Install, USB\VID_0482&PID_06c5&MI_01
Kyocera TASKalfa 7052ci = USB_Install, USB\VID_0482&PID_06c5&MI_02
Kyocera TASKalfa 8002i = USB_Install, USB\VID_0482&PID_06c6&MI_01
Kyocera TASKalfa 8002i = USB_Install, USB\VID_0482&PID_06c6&MI_02
Kyocera TASKalfa 8052ci = USB_Install, USB\VID_0482&PID_06c4&MI_01
Kyocera TASKalfa 8052ci = USB_Install, USB\VID_0482&PID_06c4&MI_02
Kyocera ECOSYS M5525cdn = USB_Install, USB\VID_0482&PID_0c16&MI_02
Kyocera ECOSYS M5520cdw = USB_Install, USB\VID_0482&PID_0c17&MI_02
Kyocera ECOSYS M5520cdn = USB_Install, USB\VID_0482&PID_0c18&MI_02
Kyocera ECOSYS P5025cdn = USB_Install, USB\VID_0482&PID_0c13&MI_01
Kyocera ECOSYS P5020cdw = USB_Install, USB\VID_0482&PID_0c14&MI_01
Kyocera ECOSYS P5020cdn = USB_Install, USB\VID_0482&PID_0c15&MI_01
;new
Kyocera ECOSYS P8060cdn = USB_Install, USB\VID_0482&PID_0c48&MI_01
Kyocera ECOSYS P4045dn = USB_Install, USB\VID_0482&PID_0C78&MI_01
Kyocera TASKalfa 350ci = USB_Install, USB\VID_0482&PID_0c94&MI_01
Kyocera TASKalfa 350ci = USB_Install, USB\VID_0482&PID_0c94&MI_02

[KDCWINUSB.NTamd64.6.0]
Kyocera CS 2552ci = USB_Install, USB\VID_0482&PID_06d5&MI_01
Kyocera CS 2552ci = USB_Install, USB\VID_0482&PID_06d5&MI_02
Kyocera CS 3252ci = USB_Install, USB\VID_0482&PID_06d4&MI_01
Kyocera CS 3252ci = USB_Install, USB\VID_0482&PID_06d4&MI_02
Kyocera CS 3552ci = USB_Install, USB\VID_0482&PID_0c35&MI_01
Kyocera CS 3552ci = USB_Install, USB\VID_0482&PID_0c35&MI_02
Kyocera CS 4002i = USB_Install, USB\VID_0482&PID_06d8&MI_01
Kyocera CS 4002i = USB_Install, USB\VID_0482&PID_06d8&MI_02
Kyocera CS 4052ci = USB_Install, USB\VID_0482&PID_06d3&MI_01
Kyocera CS 4052ci = USB_Install, USB\VID_0482&PID_06d3&MI_02
Kyocera CS 5002i = USB_Install, USB\VID_0482&PID_06d7&MI_01
Kyocera CS 5002i = USB_Install, USB\VID_0482&PID_06d7&MI_02
Kyocera CS 5052ci = USB_Install, USB\VID_0482&PID_06d2&MI_01
Kyocera CS 5052ci = USB_Install, USB\VID_0482&PID_06d2&MI_02
Kyocera CS 6002i = USB_Install, USB\VID_0482&PID_06d6&MI_01
Kyocera CS 6002i = USB_Install, USB\VID_0482&PID_06d6&MI_02
Kyocera CS 6052ci = USB_Install, USB\VID_0482&PID_06d1&MI_01
Kyocera CS 6052ci = USB_Install, USB\VID_0482&PID_06d1&MI_02
Kyocera CS 7002i = USB_Install, USB\VID_0482&PID_06dc&MI_01
Kyocera CS 7002i = USB_Install, USB\VID_0482&PID_06dc&MI_02
Kyocera CS 7052ci = USB_Install, USB\VID_0482&PID_06da&MI_01
Kyocera CS 7052ci = USB_Install, USB\VID_0482&PID_06da&MI_02
Kyocera CS 8002i = USB_Install, USB\VID_0482&PID_06db&MI_01
Kyocera CS 8002i = USB_Install, USB\VID_0482&PID_06db&MI_02
Kyocera CS 8052ci = USB_Install, USB\VID_0482&PID_06d9&MI_01
Kyocera CS 8052ci = USB_Install, USB\VID_0482&PID_06d9&MI_02
Kyocera ECOSYS M2040dn = USB_Install, USB\VID_0482&PID_069d&MI_02
Kyocera ECOSYS M2135dn = USB_Install, USB\VID_0482&PID_069a&MI_02
Kyocera ECOSYS M2540dn = USB_Install, USB\VID_0482&PID_06fd&MI_02
Kyocera ECOSYS M2540dw = USB_Install, USB\VID_0482&PID_069e&MI_02
Kyocera ECOSYS M2635dn = USB_Install, USB\VID_0482&PID_069b&MI_02
Kyocera ECOSYS M2635dw = USB_Install, USB\VID_0482&PID_069c&MI_02
Kyocera ECOSYS M2640idw = USB_Install, USB\VID_0482&PID_069f&MI_02
Kyocera ECOSYS M2735dw = USB_Install, USB\VID_0482&PID_06fe&MI_02
Kyocera ECOSYS M5520cdn = USB_Install, USB\VID_0482&PID_0c18&MI_02
Kyocera ECOSYS M5520cdw = USB_Install, USB\VID_0482&PID_0c17&MI_02
Kyocera ECOSYS M5521cdn = USB_Install, USB\VID_0482&PID_06b1&MI_02
Kyocera ECOSYS M5521cdw = USB_Install, USB\VID_0482&PID_06b2&MI_02
Kyocera ECOSYS M5525cdn = USB_Install, USB\VID_0482&PID_0c16&MI_02
Kyocera ECOSYS M5526cdn = USB_Install, USB\VID_0482&PID_06b3&MI_02
Kyocera ECOSYS M5526cdw = USB_Install, USB\VID_0482&PID_06b4&MI_02
Kyocera ECOSYS P2040dn = USB_Install, USB\VID_0482&PID_0698&MI_01
Kyocera ECOSYS P2040dw = USB_Install, USB\VID_0482&PID_0699&MI_01
Kyocera ECOSYS P2235dn = USB_Install, USB\VID_0482&PID_0696&MI_01
Kyocera ECOSYS P2235dw = USB_Install, USB\VID_0482&PID_0697&MI_01
Kyocera ECOSYS P3045dn = USB_Install, USB\VID_0482&PID_0c2d&MI_01
Kyocera ECOSYS P3050dn = USB_Install, USB\VID_0482&PID_0c2c&MI_01
Kyocera ECOSYS P3055dn = USB_Install, USB\VID_0482&PID_0c2b&MI_01
Kyocera ECOSYS P3060dn = USB_Install, USB\VID_0482&PID_0c2a&MI_01
Kyocera ECOSYS P5020cdn = USB_Install, USB\VID_0482&PID_0c15&MI_01
Kyocera ECOSYS P5020cdw = USB_Install, USB\VID_0482&PID_0c14&MI_01
Kyocera ECOSYS P5021cdn = USB_Install, USB\VID_0482&PID_06ad&MI_01
Kyocera ECOSYS P5021cdw = USB_Install, USB\VID_0482&PID_06ae&MI_01
Kyocera ECOSYS P5025cdn = USB_Install, USB\VID_0482&PID_0c13&MI_01
Kyocera ECOSYS P5026cdn = USB_Install, USB\VID_0482&PID_06af&MI_01
Kyocera ECOSYS P5026cdw = USB_Install, USB\VID_0482&PID_06b0&MI_01
Kyocera TASKalfa 2552ci = USB_Install, USB\VID_0482&PID_06c1&MI_01
Kyocera TASKalfa 2552ci = USB_Install, USB\VID_0482&PID_06c1&MI_02
Kyocera TASKalfa 3252ci = USB_Install, USB\VID_0482&PID_06c0&MI_01
Kyocera TASKalfa 3252ci = USB_Install, USB\VID_0482&PID_06c0&MI_02
Kyocera TASKalfa 3552ci = USB_Install, USB\VID_0482&PID_0c34&MI_01
Kyocera TASKalfa 3552ci = USB_Install, USB\VID_0482&PID_0c34&MI_02
Kyocera TASKalfa 4002i = USB_Install, USB\VID_0482&PID_06d0&MI_01
Kyocera TASKalfa 4002i = USB_Install, USB\VID_0482&PID_06d0&MI_02
Kyocera TASKalfa 4052ci = USB_Install, USB\VID_0482&PID_06bf&MI_01
Kyocera TASKalfa 4052ci = USB_Install, USB\VID_0482&PID_06bf&MI_02
Kyocera TASKalfa 5002i = USB_Install, USB\VID_0482&PID_06c3&MI_01
Kyocera TASKalfa 5002i = USB_Install, USB\VID_0482&PID_06c3&MI_02
Kyocera TASKalfa 5052ci = USB_Install, USB\VID_0482&PID_06be&MI_01
Kyocera TASKalfa 5052ci = USB_Install, USB\VID_0482&PID_06be&MI_02
Kyocera TASKalfa 6002i = USB_Install, USB\VID_0482&PID_06c2&MI_01
Kyocera TASKalfa 6002i = USB_Install, USB\VID_0482&PID_06c2&MI_02
Kyocera TASKalfa 6052ci = USB_Install, USB\VID_0482&PID_06bd&MI_01
Kyocera TASKalfa 6052ci = USB_Install, USB\VID_0482&PID_06bd&MI_02
Kyocera TASKalfa 7002i = USB_Install, USB\VID_0482&PID_06c7&MI_01
Kyocera TASKalfa 7002i = USB_Install, USB\VID_0482&PID_06c7&MI_02
Kyocera TASKalfa 7052ci = USB_Install, USB\VID_0482&PID_06c5&MI_01
Kyocera TASKalfa 7052ci = USB_Install, USB\VID_0482&PID_06c5&MI_02
Kyocera TASKalfa 8002i = USB_Install, USB\VID_0482&PID_06c6&MI_01
Kyocera TASKalfa 8002i = USB_Install, USB\VID_0482&PID_06c6&MI_02
Kyocera TASKalfa 8052ci = USB_Install, USB\VID_0482&PID_06c4&MI_01
Kyocera TASKalfa 8052ci = USB_Install, USB\VID_0482&PID_06c4&MI_02
Kyocera ECOSYS M5525cdn = USB_Install, USB\VID_0482&PID_0c16&MI_02
Kyocera ECOSYS M5520cdw = USB_Install, USB\VID_0482&PID_0c17&MI_02
Kyocera ECOSYS M5520cdn = USB_Install, USB\VID_0482&PID_0c18&MI_02
Kyocera ECOSYS P5025cdn = USB_Install, USB\VID_0482&PID_0c13&MI_01
Kyocera ECOSYS P5020cdw = USB_Install, USB\VID_0482&PID_0c14&MI_01
Kyocera ECOSYS P5020cdn = USB_Install, USB\VID_0482&PID_0c15&MI_01
;new
Kyocera ECOSYS P8060cdn = USB_Install, USB\VID_0482&PID_0c48&MI_01
Kyocera ECOSYS P4045dn = USB_Install, USB\VID_0482&PID_0C78&MI_01
Kyocera TASKalfa 350ci = USB_Install, USB\VID_0482&PID_0c94&MI_01
Kyocera TASKalfa 350ci = USB_Install, USB\VID_0482&PID_0c94&MI_02

; ========== Class definition ===========

[ClassInstall32]
AddReg = ClassInstall_AddReg

[ClassInstall_AddReg]
HKR,,,,%ClassName%
HKR,,NoInstallClass,,1
HKR,,IconPath,%REG_MULTI_SZ%,"%%systemroot%%\system32\setupapi.dll,-20"
HKR,,LowerLogoVersion,,5.2

; =================== Installation ===================

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include =winusb.inf
Needs   = WINUSB.NT.Services

[USB_Install.HW]
AddReg=Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{9f543223-cede-4fa3-b376-a25ce9a30e74}"


; [DestinationDirs]
; If your INF needs to copy files, you must not use the DefaultDestDir directive here.  
; You must explicitly reference all file-list-section names in this section.

; =================== Strings ===================

[Strings]
ManufacturerName="KYOCERA Document Solutions Inc."
ClassName="Universal Serial Bus devices"
DeviceName="Kyocera WINUSB"
REG_MULTI_SZ = 0x00010000

