
[Version]
Provider = Kyocera
Version  = 07/31/2017,7.2.0731

[Information]
PackageKey = KX
PackageType = KXDRV
Name = "KX DRIVER"
Description = %KXDRV_DESC%
Location = 
Category = DRIVER
MinOSVersion = 5.0
MaxOSVersion = 10.0
Connection = 
Attribute = HASPROPERTY
Required = SNMPCO,KMWINUSB1
Handler = DriverDll.dll
ProductVersion = BY_PRN_CONFIG,%INF_PATH%

[Information.FS-1100]
Required = SNMPCO,CONFIGTOOL

[Information.FS-1300D]
Required = SNMPCO,CONFIGTOOL

[Information.FS-1120D]
Required = SNMPCO,CONFIGTOOL

[Information.FS-1320D]
Required = SNMPCO,CONFIGTOOL

[Information.FS-1110]
Required = SNMPCO,CONFIGTOOL

[Information.ECOSYS P2035d]
Required = SNMPCO,CONFIGTOOL

[Information.ECOSYS P2135d]
Required = SNMPCO,CONFIGTOOL

[Default]
PrinterName = <PrinterName>
DriverName = <DriverName>
SharedName = <SharedName>
PortName = <PortName>
SharePrinter = 0
SetAsDefault = 1
PrintTestPage = 0
KACT = 1
QuickPrint = 1
StatusMonitor = 1,5
StatusMonitorNotice = 1
EnableDuplex = 1
Telemetry = 1

[Default.nt6]
PrinterName = <PrinterName>
DriverName = <DriverName>
SharedName = <SharedName>
PortName = <PortName>
SharePrinter = 0
SetAsDefault = 1
PrintTestPage = 0
KACT = 0
QuickPrint = 1
StatusMonitor = 1,5
StatusMonitorNotice = 1
EnableDuplex = 1

[Default.CS 2552ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 3252ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 3552ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 4052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 5052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 6052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 7052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 8052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5521cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5521cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5526cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5526cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5021cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5021cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5026cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5026cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.FS-C8525MFP.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 2552ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 3252ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 3552ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 4052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 5052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 6052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 7052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 8052ci.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
; new
[Default.ECOSYS M5525cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5520cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5520cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5025cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5020cdw.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5020cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M8024cidn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P8060cdn.00c0]
ChinaRed = 1,"<System32>\spool\drivers\W32X86\3\KMCR*.DLL","Utility\PostInst"


[Default.CS 2552ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 3252ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 3552ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 4052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 5052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 6052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 7052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.CS 8052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5521cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5521cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5526cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5526cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5021cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5021cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5026cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5026cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.FS-C8525MFP.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 2552ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 3252ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 3552ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 4052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 5052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 6052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 7052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.TASKalfa 8052ci.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"

; new
[Default.ECOSYS M5525cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5520cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M5520cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5025cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5020cdw.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P5020cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS M8024cidn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"
[Default.ECOSYS P8060cdn.x64.00c0]
ChinaRed = 1,"<System32>\spool\drivers\x64\3\KMCR*.DLL","Utility\PostInst"

[Options]
QuickPrintAttribute = HIDE, 2
StatusMonitorAttribute = HIDE

[Private]
Inf = ".\32bit\7 and newer\oemsetup.inf"
Inf64 = ".\64bit\7 and newer\oemsetup.inf"

[Private.x64]
Inf = ".\64bit\7 and newer\oemsetup.inf"
Inf32 = ".\32bit\7 and newer\oemsetup.inf"

[StatusMonitor]
FS-4020DN,"4X","",TCPIP,USB
FS-2020D,"4X","",TCPIP,USB
FS-3920DN,"4X","",TCPIP,USB
FS-6970DN,"4X","",TCPIP,USB
FS-1100,"4X","",TCPIP,USB
FS-1300D,"4X","",TCPIP,USB
TASKalfa 500ci,"4X","",TCPIP,USB
TASKalfa 400ci,"4X","",TCPIP,USB
TASKalfa 300ci,"4X","",TCPIP,USB
TASKalfa 250ci,"4X","",TCPIP,USB
CS 500ci,"4X","",TCPIP,USB
CS 400ci,"4X","",TCPIP,USB
CS 300ci,"4X","",TCPIP,USB
CS 250ci,"4X","",TCPIP,USB
FS-C5100DN,"4X","",TCPIP,USB
FS-C5200DN,"4X","",TCPIP,USB
FS-C5300DN,"4X","",TCPIP,USB
FS-C5400DN,"4X","",TCPIP,USB
FS-C5350DN,"4X","",TCPIP,USB
FS-1350DN,"4X","",TCPIP,USB
TASKalfa 620,"4X","",TCPIP
TASKalfa 820,"4X","",TCPIP
CS 620,"4X","",TCPIP
CS 820,"4X","",TCPIP
TASKalfa 181,"4X","",TCPIP
TASKalfa 221,"4X","",TCPIP
CS 181,"4X","",TCPIP
CS 221,"4X","",TCPIP
FS-1028MFP,"4X","",TCPIP,USB
FS-1128MFP,"4X","",TCPIP,USB
KM-2810,"4X","",TCPIP,USB
KM-2820,"4X","",TCPIP,USB
TASKalfa 552ci,"4X","",TCPIP,USB
CS 552ci,"4X","",TCPIP,USB
FS-C8500DN,"4X","",TCPIP,USB
TASKalfa 300i,"4X","",TCPIP,USB
CS 300i,"4X","",TCPIP,USB
TASKalfa 420i,"4X","",TCPIP,USB
TASKalfa 520i,"4X","",TCPIP,USB
CS 420i,"4X","",TCPIP,USB
CS 520i,"4X","",TCPIP,USB
FS-2025D,"4X","",TCPIP,USB
FS-3925DN,"4X","",TCPIP,USB
FS-4025DN,"4X","",TCPIP,USB
FS-6975DN,"4X","",TCPIP,USB
FS-1120D,"4X","",TCPIP,USB
FS-1320D,"4X","",TCPIP,USB
FS-1370DN,"4X","",TCPIP,USB
FS-3040MFP,"4X","",TCPIP,USB
FS-3140MFP,"4X","",TCPIP,USB
FS-C2026MFP,"4X","",TCPIP,USB
FS-C2126MFP,"4X","",TCPIP,USB
FS-C5150DN,"4X","",TCPIP,USB
FS-C5250DN,"4X","",TCPIP,USB
FS-6025MFP,"4X","",TCPIP,USB
FS-6030MFP,"4X","",TCPIP,USB
TASKalfa 255,"4X","",TCPIP,USB
TASKalfa 305,"4X","",TCPIP,USB
CS 255,"4X","",TCPIP,USB
CS 305,"4X","",TCPIP,USB
FS-C8020MFP,"4X","",TCPIP,USB
FS-C8025MFP,"4X","",TCPIP,USB
TASKalfa 205c,"4X","",TCPIP,USB
TASKalfa 255c,"4X","",TCPIP,USB
CS 205c,"4X","",TCPIP,USB
CS 255c,"4X","",TCPIP,USB
TASKalfa 3050ci,"4X","",TCPIP,USB
TASKalfa 3550ci,"4X","",TCPIP,USB
TASKalfa 4550ci,"4X","",TCPIP,USB
TASKalfa 5550ci,"4X","",TCPIP,USB
CS 3050ci,"4X","",TCPIP,USB
CS 3550ci,"4X","",TCPIP,USB
CS 4550ci,"4X","",TCPIP,USB
CS 5550ci,"4X","",TCPIP,USB
CS 6550ci,"4X","",TCPIP,USB
CS 7550ci,"4X","",TCPIP,USB
TASKalfa 6550ci,"4X","",TCPIP,USB
TASKalfa 7550ci,"4X","",TCPIP,USB
TASKalfa 3500i,"4X","",TCPIP,USB
TASKalfa 4500i,"4X","",TCPIP,USB
TASKalfa 5500i,"4X","",TCPIP,USB
CS 3500i,"4X","",TCPIP,USB
CS 4500i,"4X","",TCPIP,USB
CS 5500i,"4X","",TCPIP,USB
CS 6500i,"4X","",TCPIP,USB
CS 8000i,"4X","",TCPIP,USB
TASKalfa 6500i,"4X","",TCPIP,USB
TASKalfa 8000i,"4X","",TCPIP,USB
FS-C2526MFP,"4X","",TCPIP,USB
FS-C2626MFP,"4X","",TCPIP,USB
FS-3540MFP,"4X","",TCPIP,USB
FS-3640MFP,"4X","",TCPIP,USB
FS-C2026MFP+,"4X","",TCPIP,USB
FS-C2126MFP+,"4X","",TCPIP,USB
FS-3040MFP+,"4X","",TCPIP,USB
FS-3140MFP+,"4X","",TCPIP,USB
FS-1030MFP,"4X","",TCPIP,USB
FS-1130MFP,"4X","",TCPIP,USB
FS-1035MFP,"4X","",TCPIP,USB
FS-1135MFP,"4X","",TCPIP,USB
TASKalfa 2550ci,"4X","",TCPIP,USB
FS-6525MFP,"4X","",TCPIP,USB
FS-6530MFP,"4X","",TCPIP,USB
FS-C8520MFP,"4X","",TCPIP,USB
FS-C8525MFP,"4X","",TCPIP,USB
FS-C8650DN,"4X","",TCPIP,USB
FS-C8600DN,"4X","",TCPIP,USB
FS-4300DN,"4X","",TCPIP,USB
FS-4200DN,"4X","",TCPIP,USB
FS-4100DN,"4X","",TCPIP,USB
FS-2100DN,"4X","",TCPIP,USB
FS-2100D,"4X","",TCPIP,USB
CS 2550ci,"4X","",TCPIP,USB
FS-1110,"",USB
FS-1024MFP,"",USB
FS-1124MFP,"",USB
FS-C8650DN,"4X","",TCPIP,USB
FS-C8600DN,"4X","",TCPIP,USB
TASKalfa 265ci,"4X","",TCPIP,USB
TASKalfa 2551ci,"4X","",TCPIP,USB
CS 2551ci,"4X","",TCPIP,USB
TASKalfa 3510i,"4X","",TCPIP,USB
TASKalfa 3010i,"4X","",TCPIP,USB
CS 3510i,"4X","",TCPIP,USB
CS 3010i,"4X","",TCPIP,USB
TASKalfa 3051ci,"4X","",TCPIP,USB
TASKalfa 3551ci,"4X","",TCPIP,USB
TASKalfa 4551ci,"4X","",TCPIP,USB
TASKalfa 5551ci,"4X","",TCPIP,USB
CS 3051ci,"4X","",TCPIP,USB
CS 3551ci,"4X","",TCPIP,USB
CS 4551ci,"4X","",TCPIP,USB
CS 5551ci,"4X","",TCPIP,USB
CS 6551ci,"4X","",TCPIP,USB
CS 7551ci,"4X","",TCPIP,USB
TASKalfa 6551ci,"4X","",TCPIP,USB
TASKalfa 7551ci,"4X","",TCPIP,USB
TASKalfa 3501i,"4X","",TCPIP,USB
TASKalfa 4501i,"4X","",TCPIP,USB
TASKalfa 5501i,"4X","",TCPIP,USB
CS 3501i,"4X","",TCPIP,USB
CS 4501i,"4X","",TCPIP,USB
CS 5501i,"4X","",TCPIP,USB
CS 6501i,"4X","",TCPIP,USB
CS 8001i,"4X","",TCPIP,USB
TASKalfa 6501i,"4X","",TCPIP,USB
TASKalfa 8001i,"4X","",TCPIP,USB
ECOSYS M2030dn,"",TCPIP,USB
ECOSYS M2530dn,"",TCPIP,USB
ECOSYS M2035dn,"",TCPIP,USB
ECOSYS M2535dn,"",TCPIP,USB
ECOSYS M6026cdn,"",TCPIP,USB
ECOSYS M6526cdn,"",TCPIP,USB
ECOSYS M6026cidn,"",TCPIP,USB
ECOSYS M6526cidn,"",TCPIP,USB
TASKalfa 266ci,"",TCPIP,USB
ECOSYS P6021cdn,"",TCPIP,USB
ECOSYS P6026cdn,"",TCPIP,USB
ECOSYS P6030cdn,"",TCPIP,USB
ECOSYS P2035d,"4X",TCPIP,USB
ECOSYS P2135d,"4X",TCPIP,USB
ECOSYS P2135dn,"",TCPIP,USB
ECOSYS P7035cdn,"",TCPIP,USB
ECOSYS M3040dn,"",TCPIP,USB
ECOSYS M3540dn,"",TCPIP,USB
ECOSYS M3040idn,"",TCPIP,USB
ECOSYS M3540idn,"",TCPIP,USB
ECOSYS M3550idn,"",TCPIP,USB
ECOSYS M3560idn,"",TCPIP,USB
ECOSYS P6130cdn,"",TCPIP,USB
ECOSYS P6035cdn,"",TCPIP,USB
ECOSYS P7040cdn,"",TCPIP,USB
ECOSYS M6030cdn,"",TCPIP,USB
ECOSYS M6530cdn,"",TCPIP,USB
ECOSYS M6035cidn,"",TCPIP,USB
ECOSYS M6535cidn,"",TCPIP,USB
ECOSYS P4040dn,"",TCPIP,USB
ECOSYS P4035dn,"",TCPIP,USB
TASKalfa 306ci,"",TCPIP,USB
TASKalfa 356ci,"",TCPIP,USB
TASKalfa 406ci,"",TCPIP,USB
CS 306ci,"",TCPIP,USB
CS 356ci,"",TCPIP,USB
CS 406ci,"",TCPIP,USB
ECOSYS P2235dn,"",TCPIP,USB
ECOSYS P2040dn,"",TCPIP,USB
ECOSYS M2135dn,"",TCPIP,USB
ECOSYS M2635dn,"",TCPIP,USB
ECOSYS M2040dn,"",TCPIP,USB
ECOSYS M2540dn,"",TCPIP,USB
ECOSYS P2235dw,"",TCPIP,USB
ECOSYS P2040dw,"",TCPIP,USB
ECOSYS M2635dw,"",TCPIP,USB
ECOSYS M2540dw,"",TCPIP,USB
ECOSYS M2735dw,"",TCPIP,USB
ECOSYS M2640idw,"",TCPIP,USB
TASKalfa 6052ci,"",TCPIP,USB
TASKalfa 5052ci,"",TCPIP,USB
TASKalfa 4052ci,"",TCPIP,USB
TASKalfa 3552ci,"",TCPIP,USB
TASKalfa 3252ci,"",TCPIP,USB
TASKalfa 2552ci,"",TCPIP,USB
CS 6052ci,"",TCPIP,USB
CS 5052ci,"",TCPIP,USB
CS 4052ci,"",TCPIP,USB
CS 3552ci,"",TCPIP,USB
CS 3252ci,"",TCPIP,USB
CS 2552ci,"",TCPIP,USB
TASKalfa 6002i,"",TCPIP,USB
TASKalfa 5002i,"",TCPIP,USB
TASKalfa 4002i,"",TCPIP,USB
CS 6002i,"",TCPIP,USB
CS 5002i,"",TCPIP,USB
CS 4002i,"",TCPIP,USB
TASKalfa 3511i,"",TCPIP,USB
TASKalfa 3011i,"",TCPIP,USB
CS 3511i,"",TCPIP,USB
CS 3011i,"",TCPIP,USB
ECOSYS M5521cdn,"",TCPIP,USB
ECOSYS M5521cdw,"",TCPIP,USB
ECOSYS M5526cdn,"",TCPIP,USB
ECOSYS M5526cdw,"",TCPIP,USB
ECOSYS P5021cdn,"",TCPIP,USB
ECOSYS P5021cdw,"",TCPIP,USB
ECOSYS P5026cdn,"",TCPIP,USB
ECOSYS P5026cdw,"",TCPIP,USB
TASKalfa 8052ci,"",TCPIP,USB
TASKalfa 7052ci,"",TCPIP,USB
TASKalfa 8002i,"",TCPIP,USB
TASKalfa 7002i,"",TCPIP,USB
CS 8052ci,"",TCPIP,USB
CS 7052ci,"",TCPIP,USB
CS 8002i,"",TCPIP,USB
CS 7002i,"",TCPIP,USB
ECOSYS M4032idn,"",TCPIP,USB
ECOSYS M4025idn,"",TCPIP,USB
ECOSYS P3060dn,"",TCPIP,USB
ECOSYS P3055dn,"",TCPIP,USB
ECOSYS P3050dn,"",TCPIP,USB
ECOSYS P3045dn,"",TCPIP,USB
ECOSYS M5525cdn,"",TCPIP,USB
ECOSYS M5520cdw,"",TCPIP,USB
ECOSYS M5520cdn,"",TCPIP,USB
ECOSYS P5025cdn,"",TCPIP,USB
ECOSYS P5020cdw,"",TCPIP,USB
ECOSYS P5020cdn,"",TCPIP,USB
ECOSYS M8024cidn,"4X","",TCPIP,USB
ECOSYS M4028idn,"4X","",TCPIP,USB
ECOSYS P8060cdn,"",TCPIP,USB
ECOSYS P4045dn,"",TCPIP,USB
TASKalfa 350ci,"",TCPIP,USB

[StatusMonitorNotice]
TASKalfa 3050ci,"",TCPIP,USB
TASKalfa 3550ci,"",TCPIP,USB
TASKalfa 4550ci,"",TCPIP,USB
TASKalfa 5550ci,"",TCPIP,USB
CS 3050ci,"",TCPIP,USB
CS 3550ci,"",TCPIP,USB
CS 4550ci,"",TCPIP,USB
CS 5550ci,"",TCPIP,USB
CS 6550ci,"",TCPIP,USB
CS 7550ci,"",TCPIP,USB
TASKalfa 6550ci,"",TCPIP,USB
TASKalfa 7550ci,"",TCPIP,USB
TASKalfa 3500i,"",TCPIP,USB
TASKalfa 4500i,"",TCPIP,USB
TASKalfa 5500i,"",TCPIP,USB
CS 3500i,"",TCPIP,USB
CS 4500i,"",TCPIP,USB
CS 5500i,"",TCPIP,USB
CS 6500i,"",TCPIP,USB
CS 8000i,"",TCPIP,USB
TASKalfa 6500i,"",TCPIP,USB
TASKalfa 8000i,"",TCPIP,USB
TASKalfa 3051ci,"",TCPIP,USB
TASKalfa 3551ci,"",TCPIP,USB
TASKalfa 4551ci,"",TCPIP,USB
TASKalfa 5551ci,"",TCPIP,USB
CS 3051ci,"",TCPIP,USB
CS 3551ci,"",TCPIP,USB
CS 4551ci,"",TCPIP,USB
CS 5551ci,"",TCPIP,USB
CS 6551ci,"",TCPIP,USB
CS 7551ci,"",TCPIP,USB
TASKalfa 6551ci,"",TCPIP,USB
TASKalfa 7551ci,"",TCPIP,USB
TASKalfa 3501i,"",TCPIP,USB
TASKalfa 4501i,"",TCPIP,USB
TASKalfa 5501i,"",TCPIP,USB
CS 3501i,"",TCPIP,USB
CS 4501i,"",TCPIP,USB
CS 5501i,"",TCPIP,USB
CS 6501i,"",TCPIP,USB
CS 8001i,"",TCPIP,USB
TASKalfa 6501i,"",TCPIP,USB
TASKalfa 8001i,"",TCPIP,USB
TASKalfa 2551ci,"",TCPIP,USB
CS 2551ci,"",TCPIP,USB
TASKalfa 3510i,"",TCPIP,USB
TASKalfa 3010i,"",TCPIP,USB
CS 3510i,"",TCPIP,USB
CS 3010i,"",TCPIP,USB
FS-C8650DN,"",TCPIP,USB
FS-C8600DN,"",TCPIP,USB

[EnableDuplex]
ALL
FS-820,EXCLUDE
FS-920,EXCLUDE
FS-1010,EXCLUDE
FS-1050,EXCLUDE
FS-1100,EXCLUDE
FS-1110,EXCLUDE
FS-1018MFP,EXCLUDE
KM-1815,EXCLUDE
CS-1815,EXCLUDE
FS-1118MFP,EXCLUDE
KM-1820,EXCLUDE
CS-1820,EXCLUDE
FS-1024MFP,EXCLUDE
FS-1124MFP,EXCLUDE
KM-1530,EXCLUDE



[TargetPath]

[Install]

[Remove]

[Verify]
VerifyDriver = KxVer

[Verify.addi]
VerifyDriver = KxVerAddi

[KxVer]
; CompareVersion = COMMAND,"INF file for the driver"
;			COMMAND = VERIFY_PRN_CONFIG,VERIFY_PRN_DATA
;     TARGET_FILE = DRV_DRIVER,DRV_CONFIG
CompareVersion = VERIFY_PRN_CONFIG,".\32bit\7 and newer\oemsetup.inf"

[KxVer.x64]
CompareVersion = VERIFY_PRN_CONFIG,".\64bit\7 and newer\oemsetup.inf"

[KxVerAddi]
CompareVersion = VERIFY_PRN_CONFIG,".\64bit\7 and newer\oemsetup.inf"

[KxVerAddi.x64]
CompareVersion = VERIFY_PRN_CONFIG,".\32bit\7 and newer\oemsetup.inf"

[Strings]
INF_PATH = ".\32bit\7 and newer\oemsetup.inf" 

[Strings.x64]
INF_PATH = ".\64bit\7 and newer\oemsetup.inf" 

[Strings.u]
KXDRV_DESC = "(Recommended) Extended-functionality printing"

;English
[Strings.u.0009]
KXDRV_DESC = "(Recommended) Extended-functionality printing"

;French
[Strings.u.000c]
KXDRV_DESC = "(recommandé) Impression Fonctionnalités étendues"

;Germany
[Strings.u.0007]
KXDRV_DESC = "(Empfohlen) Drucken mit erweiterter Funktionalität"

;Italian
[Strings.u.0010]
KXDRV_DESC = "(consigliata) Stampa con funzionalità estese"

;Japanese
[Strings.u.0011]
KXDRV_DESC = "(推奨)拡張機能印刷をサポートします"

;korean
[Strings.u.0012]
KXDRV_DESC = "(권장)인쇄 확장 기능"

;PortugueBrazil
[Strings.u.0016]
KXDRV_DESC = "(Recomendado) Impressão de funcionalidade estendida"

;SpanishIntl
[Strings.u.000a]
KXDRV_DESC = "(recomendado) Impresión con funcionalidad ampliada"

;Czech
[Strings.u.0005]
KXDRV_DESC = "(doporučeno) Rozšířená funkce tisku"

;Russian
[Strings.u.0019]
KXDRV_DESC = "(рекомендуется) Печать с расширенными функциями"

;Dutch
[Strings.u.0013]
KXDRV_DESC = "(aanbevolen) Afdrukken met uitgebreide functionaliteit"

;Polish
[Strings.u.0015]
KXDRV_DESC = "(zalecane) Drukowanie z dodatkowymi funkcjami"

;SChinese
[Strings.u.00c0]
KXDRV_DESC = "（推荐）扩展功能打印"

;TChinese
[Strings.u.00c1]
KXDRV_DESC = "(建議)延伸功能列印"

;Swedish
[Strings.u.001d]
KXDRV_DESC = "(rekommenderas)Utskrift med utökade funktioner"

;Norwegian
[Strings.u.0014]
KXDRV_DESC = "(Anbefales) Utskrift med utvidet funksjonalitet"

;Hungarian
[Strings.u.000e]
KXDRV_DESC = "(ajánlott) Bővített funkciós nyomtatás"

;Finnish
[Strings.u.000b]
KXDRV_DESC = "(suositellaan) Tulostus, jossa on lisätoimintoja"

;Greek
[Strings.u.0008]
KXDRV_DESC = "(Συνιστάται) Εκτύπωση εκτεταμένης λειτουργικότητας"

;Turkish
[Strings.u.001f]
KXDRV_DESC = "(Önerilen) Genişletilmiş işlevsellik yazdırma"

;Danish
[Strings.u.0006]
KXDRV_DESC = "(anbefalet) Udskrivning med udvidede funktioner"

;Por_Portugal
[Strings.u.0816]
KXDRV_DESC = "(Recomendada) Impressão com funcionalidade avançada"

;Hebrew
[Strings.u.000d]
KXDRV_DESC = "(מומלץ) הדפסה בתפקודיות מורחבת"

;Romanian
[Strings.u.0018]
KXDRV_DESC = "(Recomandat) Imprimare cu funcţionalitate extinsă"

;Arabic
[Strings.u.0001]
KXDRV_DESC = "(موصى به) طباعة الوظائف الممتدة"

;Catalan
[Strings.u.0003]
KXDRV_DESC = "(Recomanat) Funcionalitat d'impressió ampliada"

;Thai
[Strings.u.001e]
KXDRV_DESC = "(แนะนำ) การพิมพ์ที่เพิ่มความสามารถในการทำงาน "

;Vietnamese
[Strings.u.002a]
KXDRV_DESC = "(Nên dùng) Chế độ in với chức năng mở rộng"

